(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Amplifier_Audio:LM386" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 7.62 0))
      (property "Value" "LM386" (id 1) (at 1.27 5.08 0))
      (property "Footprint" "" (id 2) (at 2.54 2.54 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf" (id 3) (at 5.08 5.08 0))
      (property "ki_keywords" "single Power opamp" (id 4) (at 0 0 0))
      (property "ki_description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSSOP*P0.65mm* TSSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "LM386_0_1"
        (polyline
          (pts
            (xy 5.08 0)
            (xy -5.08 5.08)
            (xy -5.08 -5.08)
            (xy 5.08 0)
          )
          (fill (type background))
        )
      )
      (symbol "LM386_1_1"
        (pin input line (at 0 -7.62 90) (length 5.08)
          (name "GAIN")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "3")
        )
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "GND")
          (number "4")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "6")
        )
        (pin input line (at 0 7.62 270) (length 5.08)
          (name "BYPASS")
          (number "7")
        )
        (pin input line (at 2.54 -7.62 90) (length 6.35)
          (name "GAIN")
          (number "8")
        )
      )
    )
    (symbol "Device:Battery" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (id 0) (at 2.54 2.54 0))
      (property "Value" "Battery" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 1.524 90))
      (property "Datasheet" "~" (id 3) (at 0 1.524 90))
      (property "ki_keywords" "batt voltage-source cell" (id 4) (at 0 0 0))
      (property "ki_description" "Multiple-cell battery" (id 5) (at 0 0 0))
      (symbol "Battery_0_1"
        (rectangle (start -2.032 -1.397) (end 2.032 -1.651)
          (fill (type outline))
        )
        (rectangle (start -2.032 1.778) (end 2.032 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.3208 -1.9812) (end 1.27 -2.4892)
          (fill (type outline))
        )
        (rectangle (start -1.3208 1.1938) (end 1.27 0.6858)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -1.524)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.016)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.508)
            (xy 0 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.508)
            (xy 0 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 2.667)
            (xy 1.27 2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 3.175)
            (xy 0.762 2.159)
          )
          (fill (type none))
        )
      )
      (symbol "Battery_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_Polarized" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "C_Polarized_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Microphone_Condenser" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "MK" (id 0) (at -3.302 1.27 0))
      (property "Value" "Microphone_Condenser" (id 1) (at -3.302 -0.635 0))
      (property "Footprint" "" (id 2) (at 0 2.54 90))
      (property "Datasheet" "~" (id 3) (at 0 2.54 90))
      (property "ki_keywords" "capacitance condenser microphone" (id 4) (at 0 0 0))
      (property "ki_description" "Condenser microphone" (id 5) (at 0 0 0))
      (symbol "Microphone_Condenser_0_1"
        (polyline
          (pts
            (xy -2.54 2.54)
            (xy -2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 0 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 0 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 3.81)
            (xy 0.762 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 4.064)
            (xy 0.508 3.556)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 2.54)
          (fill (type none))
        )
        (rectangle (start 1.016 -0.254) (end -1.016 -0.762)
          (fill (type outline))
        )
        (rectangle (start 1.016 0.762) (end -1.016 0.254)
          (fill (type outline))
        )
      )
      (symbol "Microphone_Condenser_1_1"
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Potentiometer" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RV" (id 0) (at -4.445 0 90))
      (property "Value" "R_Potentiometer" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "resistor variable" (id 4) (at 0 0 0))
      (property "ki_description" "Potentiometer" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Potentiometer*" (id 6) (at 0 0 0))
      (symbol "R_Potentiometer_0_1"
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.524 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 0)
            (xy 2.286 0.508)
            (xy 2.286 -0.508)
            (xy 1.143 0)
          )
          (fill (type outline))
        )
        (rectangle (start 1.016 2.54) (end -1.016 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_Potentiometer_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Device:Speaker" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "LS" (id 0) (at 1.27 5.715 0))
      (property "Value" "Speaker" (id 1) (at 1.27 3.81 0))
      (property "Footprint" "" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "~" (id 3) (at -0.254 -1.27 0))
      (property "ki_keywords" "speaker sound" (id 4) (at 0 0 0))
      (property "ki_description" "Speaker" (id 5) (at 0 0 0))
      (symbol "Speaker_0_0"
        (rectangle (start -2.54 1.27) (end 1.016 -3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 3.556 3.81)
            (xy 3.556 -6.35)
            (xy 1.016 -3.81)
          )
          (fill (type none))
        )
      )
      (symbol "Speaker_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Linear:L78L05_TO92" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "L78L05_TO92" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 0 5.715 0))
      (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf" (id 3) (at 0 -1.27 0))
      (property "ki_keywords" "Voltage Regulator 100mA Positive" (id 4) (at 0 0 0))
      (property "ki_description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, TO-92" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?92*" (id 6) (at 0 0 0))
      (symbol "L78L05_TO92_0_1"
        (rectangle (start -5.08 -5.08) (end 5.08 1.905)
          (fill (type background))
        )
      )
      (symbol "L78L05_TO92_1_1"
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "3")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "global power" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 43.18 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 67.31) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 31.75 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 67.31) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 43.18 59.69) (xy 43.18 52.07)))
  (wire (pts (xy 31.75 39.37) (xy 31.75 52.07)))
  (wire (pts (xy 54.61 72.39) (xy 54.61 67.31)))
  (wire (pts (xy 99.06 74.93) (xy 116.84 74.93)))
  (wire (pts (xy 121.92 39.37) (xy 31.75 39.37)))
  (wire (pts (xy 81.28 78.74) (xy 85.09 78.74)))
  (wire (pts (xy 43.18 67.31) (xy 54.61 67.31)))
  (wire (pts (xy 116.84 63.5) (xy 116.84 74.93)))
  (wire (pts (xy 99.06 71.12) (xy 99.06 74.93)))
  (wire (pts (xy 121.92 39.37) (xy 121.92 53.34)))
  (wire (pts (xy 92.71 67.31) (xy 95.25 67.31)))
  (wire (pts (xy 54.61 67.31) (xy 55.88 67.31)))
  (wire (pts (xy 43.18 52.07) (xy 48.26 52.07)))
  (wire (pts (xy 64.77 52.07) (xy 81.28 52.07)))
  (wire (pts (xy 81.28 90.17) (xy 81.28 93.98)))
  (wire (pts (xy 81.28 77.47) (xy 81.28 78.74)))
  (wire (pts (xy 64.77 59.69) (xy 64.77 52.07)))
  (wire (pts (xy 55.88 67.31) (xy 64.77 67.31)))
  (wire (pts (xy 161.29 60.96) (xy 175.26 60.96)))
  (wire (pts (xy 121.92 76.2) (xy 143.51 76.2)))
  (wire (pts (xy 121.92 74.93) (xy 121.92 76.2)))
  (wire (pts (xy 81.28 78.74) (xy 81.28 80.01)))
  (wire (pts (xy 132.08 60.96) (xy 143.51 60.96)))
  (wire (pts (xy 31.75 52.07) (xy 43.18 52.07)))
  (wire (pts (xy 143.51 60.96) (xy 153.67 60.96)))
  (wire (pts (xy 64.77 52.07) (xy 63.5 52.07)))
  (wire (pts (xy 99.06 63.5) (xy 99.06 58.42)))
  (wire (pts (xy 31.75 62.23) (xy 31.75 69.85)))
  (wire (pts (xy 121.92 68.58) (xy 121.92 74.93)))
  (wire (pts (xy 55.88 59.69) (xy 55.88 67.31)))
  (wire (pts (xy 175.26 63.5) (xy 175.26 76.2)))
  (wire (pts (xy 92.71 78.74) (xy 92.71 67.31)))
  (wire (pts (xy 143.51 76.2) (xy 175.26 76.2)))
  (wire (pts (xy 99.06 58.42) (xy 116.84 58.42)))
  (wire (pts (xy 81.28 52.07) (xy 81.28 69.85)))
  (wire (pts (xy 116.84 74.93) (xy 121.92 74.93)))
  (symbol (lib_id "Device:C") (at 64.77 63.5 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 68.58 62.2299 0))
    (property "Value" "1nf" (id 1) (at 68.58 64.7699 0))
    (property "Footprint" "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (id 2) (at 65.7352 67.31 0))
    (property "Datasheet" "~" (id 3) (at 64.77 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 81.28 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 83.82 72.3899 0))
    (property "Value" "10k" (id 1) (at 83.82 74.9299 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (id 2) (at 79.502 73.66 90))
    (property "Datasheet" "~" (id 3) (at 81.28 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 31.75 69.85 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0102" (id 0) (at 31.75 76.2 0))
    (property "Value" "GND" (id 1) (at 31.75 74.93 0))
    (property "Footprint" "" (id 2) (at 31.75 69.85 0))
    (property "Datasheet" "" (id 3) (at 31.75 69.85 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Microphone_Condenser") (at 81.28 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "MK1" (id 0) (at 85.09 83.1214 0))
    (property "Value" "Microphone_Condenser" (id 1) (at 85.09 85.6614 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (id 2) (at 81.28 82.55 90))
    (property "Datasheet" "~" (id 3) (at 81.28 82.55 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 43.18 63.5 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 46.99 62.2299 0))
    (property "Value" "33nf" (id 1) (at 46.99 64.7699 0))
    (property "Footprint" "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (id 2) (at 44.1452 67.31 0))
    (property "Datasheet" "~" (id 3) (at 43.18 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 81.28 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0104" (id 0) (at 81.28 100.33 0))
    (property "Value" "GND" (id 1) (at 81.28 99.06 0))
    (property "Footprint" "" (id 2) (at 81.28 93.98 0))
    (property "Datasheet" "" (id 3) (at 81.28 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "Amplifier_Audio:LM386") (at 124.46 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 134.62 56.261 0))
    (property "Value" "LM386" (id 1) (at 134.62 58.801 0))
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm_Socket" (id 2) (at 127 58.42 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf" (id 3) (at 129.54 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:C") (at 88.9 78.74 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C3" (id 0) (at 88.9 71.12 90))
    (property "Value" "1nf" (id 1) (at 88.9 73.66 90))
    (property "Footprint" "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (id 2) (at 92.71 77.7748 0))
    (property "Datasheet" "~" (id 3) (at 88.9 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized") (at 157.48 60.96 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C5" (id 0) (at 156.591 53.34 90))
    (property "Value" "470µf" (id 1) (at 156.591 55.88 90))
    (property "Footprint" "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (id 2) (at 161.29 59.9948 0))
    (property "Datasheet" "~" (id 3) (at 157.48 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 143.51 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 146.05 71.1199 0))
    (property "Value" "10" (id 1) (at 146.05 73.6599 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (id 2) (at 141.732 72.39 90))
    (property "Datasheet" "~" (id 3) (at 143.51 72.39 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Potentiometer") (at 99.06 67.31 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "RV1" (id 0) (at 101.6 66.0399 0))
    (property "Value" "470K" (id 1) (at 101.6 68.5799 0))
    (property "Footprint" "Potentiometer_THT:Potentiometer_Piher_PT-10-V05_Vertical" (id 2) (at 99.06 67.31 0))
    (property "Datasheet" "~" (id 3) (at 99.06 67.31 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Regulator_Linear:L78L05_TO92") (at 55.88 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 55.88 44.45 0))
    (property "Value" "L78L05_TO92" (id 1) (at 55.88 46.99 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline_Wide" (id 2) (at 55.88 46.355 0))
    (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf" (id 3) (at 55.88 53.34 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:Battery") (at 31.75 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "BT1" (id 0) (at 35.56 55.4989 0))
    (property "Value" "Battery" (id 1) (at 35.56 58.0389 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (id 2) (at 31.75 55.626 90))
    (property "Datasheet" "~" (id 3) (at 31.75 55.626 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Speaker") (at 180.34 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "LS1" (id 0) (at 185.42 60.9599 0))
    (property "Value" "Speaker" (id 1) (at 185.42 63.4999 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (id 2) (at 180.34 66.04 0))
    (property "Datasheet" "~" (id 3) (at 180.086 62.23 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 121.92 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0105" (id 0) (at 121.92 82.55 0))
    (property "Value" "GND" (id 1) (at 121.92 81.28 0))
    (property "Footprint" "" (id 2) (at 121.92 76.2 0))
    (property "Datasheet" "" (id 3) (at 121.92 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 143.51 64.77 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C4" (id 0) (at 147.32 63.4999 0))
    (property "Value" "47n" (id 1) (at 147.32 66.0399 0))
    (property "Footprint" "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (id 2) (at 142.5448 60.96 0))
    (property "Datasheet" "~" (id 3) (at 143.51 64.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 54.61 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0101" (id 0) (at 54.61 78.74 0))
    (property "Value" "GND" (id 1) (at 54.61 77.47 0))
    (property "Footprint" "" (id 2) (at 54.61 72.39 0))
    (property "Datasheet" "" (id 3) (at 54.61 72.39 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "BT1") (unit 1) (value "Battery") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical")
    )
    (path
      (reference "C1") (unit 1) (value "33nf") (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2")
    )
    (path
      (reference "C2") (unit 1) (value "1nf") (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2")
    )
    (path
      (reference "C3") (unit 1) (value "1nf") (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2")
    )
    (path
      (reference "C4") (unit 1) (value "47n") (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2")
    )
    (path
      (reference "C5") (unit 1) (value "470µf") (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2")
    )
    (path
      (reference "LS1") (unit 1) (value "Speaker") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical")
    )
    (path
      (reference "MK1") (unit 1) (value "Microphone_Condenser") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical")
    )
    (path
      (reference "R1") (unit 1) (value "10k") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R2") (unit 1) (value "10") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal")
    )
    (path
      (reference "RV1") (unit 1) (value "470K") (footprint "Potentiometer_THT:Potentiometer_Piher_PT-10-V05_Vertical")
    )
    (path
      (reference "U1") (unit 1) (value "L78L05_TO92") (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide")
    )
    (path
      (reference "U2") (unit 1) (value "LM386") (footprint "Package_DIP:DIP-8_W7.62mm_Socket")
    )
  )
)
