(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 "GND")
  (net 3 "VDD")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C7-Pad2)")
  (net 8 "Net-(C10-Pad2)")
  (net 9 "Net-(RV1-Pad3)")
  (net 10 "-15V")
  (net 11 "+15V")
  (net 12 "Net-(C3-Pad1)")
  (net 13 "Net-(C4-Pad1)")
  (net 14 "Net-(C4-Pad2)")
  (net 15 "Net-(C5-Pad1)")
  (net 16 "Net-(C6-Pad1)")
  (net 17 "Net-(C10-Pad1)")
  (net 18 "Net-(C9-Pad1)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "Net-(R3-Pad1)")
  (net 21 "Net-(R4-Pad1)")
  (net 22 "unconnected-(U3-Pad3)")
  (net 23 "unconnected-(U2-Pad2)")
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 105.935 114.4425)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "10uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 63.967276 80.337224)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C11" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "100uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "VDD") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 86.36 106.045)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 7.62 -2.72) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 7.62 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VDD") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 86.36 101.6)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 7.62 -2.72) (layer "F.SilkS"))
    (fp_text value "1.2K" (at 7.62 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 106.57 87.1375)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "100uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 127.969216 118.11)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "220pF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 86.255491 88.9)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 80.587276 101.022724 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 7.62 -2.72 90) (layer "F.SilkS"))
    (fp_text value "330" (at 7.62 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W10.16mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 135.88 94.595 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 10.16mm 400mil")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 5.08 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LM386" (at 5.08 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C6-Pad1)") (pinfunction "GAIN") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U2-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(RV1-Pad3)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "-15V") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 10.16 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)") (pintype "output"))
    (pad "6" thru_hole oval (at 10.16 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "7" thru_hole oval (at 10.16 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "BYPASS") (pintype "input"))
    (pad "8" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R4-Pad1)") (pinfunction "GAIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W10.16mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 105.935 107.4575)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "10uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 67.374888 106.68)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "1nF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VDD") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Battery:BatteryHolder_MPD_BH-18650-PC2" (layer "F.Cu")
    (tedit 5C1007C1)
    (at 65.6 64.77)
    (descr "18650 Battery Holder (http://www.memoryprotectiondevices.com/datasheets/BK-18650-PC2-datasheet.pdf)")
    (tags "18650 Battery Holder")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at 36 1) (layer "F.SilkS"))
    (fp_text value "Pile 9V" (at 36 -0.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 36 -2.4) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 8.645 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 64.255 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 72 0) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_MPD_BH-18650-PC2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92Flat" (layer "F.Cu")
    (tedit 5C2D433B)
    (at 60.325 93.98 90)
    (descr "TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)")
    (tags "to-92Flat hall sensor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 1.27 -1.45 90) (layer "F.SilkS"))
    (fp_text value "L78L05_TO92" (at 1.25 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0.2 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.238)
      (net 3 "VDD") (pinfunction "VO") (pintype "power_out"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W10.16mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 135.89 79.375 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 10.16mm 400mil")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 5.08 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LM386" (at 5.08 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C5-Pad1)") (pinfunction "GAIN") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(RV1-Pad3)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U3-Pad3)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "-15V") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 10.16 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C4-Pad2)") (pintype "output"))
    (pad "6" thru_hole oval (at 10.16 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "7" thru_hole oval (at 10.16 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "BYPASS") (pintype "input"))
    (pad "8" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad1)") (pinfunction "GAIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W10.16mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 66.871276 85.782724 -90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 7.62 -2.72 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 7.62 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VDD") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "mes_empreintes:2_IN_3_OUT" (layer "F.Cu")
    (tedit 0)
    (at 142.24 90.805 90)
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 -2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text value "NMA0515SC" (at 0 3.048 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "+15" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad "-15" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad "GND" thru_hole rect (at -6.35 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad "GND" thru_hole rect (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad "VDD" thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 104.775 97.155)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 7.62 -2.72) (layer "F.SilkS"))
    (fp_text value "10K" (at 7.62 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "VDD") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 127.525 109.9975)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "22uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_1.27mm:PinSocket_1x03_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 5A19A41D)
    (at 150.52 91.435)
    (descr "Through hole straight socket strip, 1x03, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 1.27mm single row")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.135) (layer "F.SilkS"))
    (fp_text value "Casque" (at 0 4.675) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(C4-Pad2)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x03_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 84.345 111.9025)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at 9 -4.12) (layer "F.SilkS"))
    (fp_text value "10uF" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 86.440216 80.772)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "33nF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA9-V10_Vertical_Hole" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 96.012 80.772 -90)
    (descr "Potentiometer, vertical, shaft hole, ACP CA9-V10, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
    (tags "Potentiometer vertical hole ACP CA9-V10")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at 5 -8.65 90) (layer "F.SilkS"))
    (fp_text value "470K" (at 5 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 -2.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 5 -2.5 270) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 10 -2.5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(RV1-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA9-V10_Vertical_Hole.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 60.96 102.235)
    (descr "Through hole straight socket strip, 1x03, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.00mm single row")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "MK1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "mic1" (at 0 6.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C3-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 104.775 101.6)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 7.62 -2.72) (layer "F.SilkS"))
    (fp_text value "1.2K" (at 7.62 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 97.155 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 7.62 -2.72) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 7.62 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-52-3_Window" (layer "F.Cu")
    (tedit 5A02FF81)
    (at 79.063276 105.594724 -90)
    (descr "TO-52-3_Window, Window")
    (tags "TO-52-3_Window Window")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -4.02 90) (layer "F.SilkS"))
    (fp_text value "BC108" (at 1.27 4.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -4.02 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 270) (size 1.6 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(C9-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(C10-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-52-3_Window.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 73.983276 101.022724 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 7.62 -2.72 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 7.62 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 134.62 118.11)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "test_Projet_Amplificator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "1nF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 161.036 51.054) (end 161.036 124.714) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 53.848 50.8) (end 161.036 51.054) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 53.086 50.8) (end 53.848 50.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 161.036 124.714) (end 53.34 124.46) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 53.34 124.46) (end 53.086 50.8) (layer "Edge.Cuts") (width 0.1))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 123.444)
        (xy 54.102 123.444)
        (xy 53.848 52.07)
        (xy 160.02 52.07)
      )
    )
  )
)
