(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(U1-Pad5)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R2-Pad2)")
  (net 11 "Net-(TH1-Pad1)")
  (footprint "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 130.048 77.216)
    (descr "VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/tlv62095.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 3.202 -2.466) (layer "F.SilkS"))
    (fp_text value "BQ24230RGT" (at 4.702 -9.966) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.42 -0.42) (size 0.73 0.73) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.42 0.42) (size 0.73 0.73) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.42 0.42) (size 0.73 0.73) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.42 -0.42) (size 0.73 0.73) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -1.4625 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(TH1-Pad1)") (pinfunction "TS") (pintype "passive"))
    (pad "2" smd roundrect (at -1.4625 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)") (pinfunction "BAT") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.4625 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)") (pinfunction "BAT") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -1.4625 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "CE") (pintype "input"))
    (pad "5" smd roundrect (at -0.75 1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad5)") (pinfunction "EN2") (pintype "input"))
    (pad "6" smd roundrect (at -0.25 1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "EN1") (pintype "input"))
    (pad "7" smd roundrect (at 0.25 1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-Pad1)") (pinfunction "PGOOD") (pintype "open_collector"))
    (pad "8" smd roundrect (at 0.75 1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect (at 1.4625 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D2-Pad1)") (pinfunction "CHG") (pintype "open_collector"))
    (pad "10" smd roundrect (at 1.4625 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad5)") (pinfunction "OUT") (pintype "power_out"))
    (pad "11" smd roundrect (at 1.4625 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad5)") (pinfunction "OUT") (pintype "passive"))
    (pad "12" smd roundrect (at 1.4625 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R1-Pad2)") (pinfunction "ILIM") (pintype "passive"))
    (pad "13" smd roundrect (at 0.75 -1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pinfunction "IN") (pintype "power_in"))
    (pad "14" smd roundrect (at 0.25 -1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "TMR") (pintype "passive"))
    (pad "15" smd roundrect (at -0.25 -1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "TD") (pintype "input"))
    (pad "16" smd roundrect (at -0.75 -1.4625) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R2-Pad2)") (pinfunction "ISET") (pintype "passive"))
    (pad "17" smd rect (at 0 0) (size 1.68 1.68) (layers "B.Cu")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" smd rect (at 0 0) (size 1.68 1.68) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" thru_hole circle (at 0.59 -0.59) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" thru_hole circle (at -0.59 -0.59) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" thru_hole circle (at 0.59 0.59) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" thru_hole circle (at -0.59 0.59) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 144.175 76.0175 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TH1" (at 8.9825 -1.825 90) (layer "F.SilkS") hide)
    (fp_text value "Thermistor" (at 3.81 2.37 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.9825 -0.075 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(TH1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_Rectangular_W5.0mm_H2.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 131.826 81.529 -90)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 2 pins")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 9.221 -0.174 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 7.721 -0.174 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_Rectangular_W5.0mm_H2.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 117.342621 69.375)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -4.092621 -4.375) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at -0.092621 -4.375) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 141.1 83.6525 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -2.37 90) (layer "F.SilkS") hide)
    (fp_text value "4.32K" (at 2.9025 0.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.6525 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 149.6 82.16 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -3.34 -1.6 180) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at -3.34 2.15 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126.8 69.3 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 3.2 -4.4) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0.5 -4.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 117.65 84.1 180)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.65 -0.9) (layer "F.SilkS"))
    (fp_text value "Connection_batterie" (at 4.65 0.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 155.975 81.685 180)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -1.56) (layer "F.SilkS"))
    (fp_text value "Connection_reste_circuit" (at -1.525 1.185 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 122.375 64.55 -90)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.85 0.575 180) (layer "F.SilkS"))
    (fp_text value "Connection USB-C" (at -1.55 -8.25 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.5) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_Rectangular_W5.0mm_H2.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 128.778 81.534 -90)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 2 pins")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 9.216 0.528 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 7.716 0.528 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_Rectangular_W5.0mm_H2.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 124.968 84.582 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -2.37 90) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 2.832 0.032 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.082 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 136 83.71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37 90) (layer "F.SilkS") hide)
    (fp_text value "2.94K" (at 2.96 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.71 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 121.412 84.582 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "circuit_charge_décharge_amplificator_V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -2.37 90) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 2.832 0.088 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.082 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 110.49 59.69) (end 160.02 59.69) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.02 93.98) (end 110.49 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.49 93.98) (end 110.49 59.69) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.02 59.69) (end 160.02 93.98) (layer "Edge.Cuts") (width 0.1))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 92.71)
        (xy 111.76 92.71)
        (xy 111.76 60.96)
        (xy 158.75 60.96)
      )
    )
  )
)
