(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-VOUT+)")
  (net 2 "Net-(U1-VOUT-)")
  (net 3 "Net-(+15-Pin_1)")
  (net 4 "Net-(5V1-Pin_1)")
  (net 5 "Net-(GND1-Pin_1)")
  (footprint "Connector_Pin:Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork" (layer "F.Cu")
    (at 77.47 68.58)
    (descr "solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "5V1" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "~" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.95) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(5V1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 77.47 81.28)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L1" (at -0.635 2.54) (layer "F.SilkS"))
    (fp_text value "100µh" (at 1.27 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.37) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-VOUT+)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02" (layer "F.Cu")
    (at 82.59 76.2)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 1.23 -1.905) (layer "F.SilkS"))
    (fp_text value "3.3µ" (at 1.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 79.375 76.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L2" (at 2.54 1.905) (layer "F.SilkS"))
    (fp_text value "100µH" (at 1.51 2.49) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.37) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork" (layer "F.Cu")
    (at 77.47 71.755)
    (descr "solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "GND1" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "~" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.95) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(GND1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02" (layer "F.Cu")
    (at 82.59 81.28)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 1.23 1.905) (layer "F.SilkS"))
    (fp_text value "3.3µ" (at 1.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork" (layer "F.Cu")
    (at 88.265 76.2)
    (descr "solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "-15" (at 0 -1.905) (layer "F.SilkS"))
    (fp_text value "~" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.95) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork" (layer "F.Cu")
    (at 88.265 81.28)
    (descr "solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "+15" (at 0 1.95) (layer "F.SilkS"))
    (fp_text value "~" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.95) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT" (layer "F.Cu")
    (at 74.045 68.81)
    (descr "Murata NMAxxxxSC footprint based on SIP7, http://power.murata.com/data/power/ncl/kdc_nma.pdf")
    (tags "Murata NMAxxxxSC DCDC-Converter")
    (property "Sheetfile" "nma0515solosboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "+/-33mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, +/-15V Output Voltage, SIP3")
    (property "ki_keywords" "Murata isolated isolation dc-dc converter")
    (attr through_hole)
    (fp_text reference "U1" (at -3 -3) (layer "F.SilkS"))
    (fp_text value "NMA0515SC" (at -1 19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.25 6 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(5V1-Pin_1)") (pinfunction "VIN+") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(GND1-Pin_1)") (pinfunction "VIN-") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(U1-VOUT-)") (pinfunction "VOUT-") (pintype "power_out"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(+15-Pin_1)") (pinfunction "0V") (pintype "power_out"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-VOUT+)") (pinfunction "VOUT+") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_NMAxxxxSC_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 90.17 66.04) (end 90.17 86.995)
    (layer "Edge.Cuts"))
  (gr_line (start 68.58 66.04) (end 90.17 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 68.58 86.995) (end 68.58 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 90.17 86.995) (end 68.58 86.995)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 68.58 66.04)
        (xy 90.17 66.04)
        (xy 90.17 86.995)
        (xy 68.58 86.995)
      )
    )
  )
)
