#!/usr/bin/env bash
#
# Build tests for LPC1768 (NXP ARM Cortex-M3)
#

# exit on first failure
set -e

#
# Build with the default configurations
#
#restore_configs
#opt_set MOTHERBOARD BOARD_RAMPS_14_RE_ARM_EFB
#exec_test $1 $2 "Default Configuration" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_RAMPS_14_RE_ARM_EFB  SERIAL_PORT_3 3 \
        NEOPIXEL_TYPE NEO_GRB RGB_LED_R_PIN P2_12 RGB_LED_G_PIN P1_23 RGB_LED_B_PIN P1_22 RGB_LED_W_PIN P1_24
opt_enable FYSETC_MINI_12864_2_1 SDSUPPORT SDCARD_READONLY SERIAL_PORT_2 RGBW_LED E_DUAL_STEPPER_DRIVERS \
           NEOPIXEL_LED NEOPIXEL_IS_SEQUENTIAL NEOPIXEL_STARTUP_TEST NEOPIXEL_BKGD_INDEX_FIRST NEOPIXEL_BKGD_INDEX_LAST NEOPIXEL_BKGD_COLOR NEOPIXEL_BKGD_ALWAYS_ON
exec_test $1 $2 "ReARM EFB VIKI2, SDSUPPORT, 2 Serial ports (USB CDC + UART0), NeoPixel" "$3"

#restore_configs
#use_example_configs Mks/Sbase
#exec_test $1 $2 "MKS SBASE Example Config" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_MKS_SBASE \
        EXTRUDERS 2 TEMP_SENSOR_1 1 \
        NUM_SERVOS 2 SERVO_DELAY '{ 300, 300 }'
opt_enable SWITCHING_NOZZLE SWITCHING_NOZZLE_E1_SERVO_NR ULTIMAKERCONTROLLER REALTIME_REPORTING_COMMANDS FULL_REPORT_TO_HOST_FEATURE
exec_test $1 $2 "MKS SBASE with SWITCHING_NOZZLE, Grbl Realtime Report" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_RAMPS_14_RE_ARM_EEB \
        EXTRUDERS 2 TEMP_SENSOR_1 -1 TEMP_SENSOR_BED 5 \
        GRID_MAX_POINTS_X 16 \
        NOZZLE_TO_PROBE_OFFSET '{ 0, 0, 0 }' \
        NOZZLE_CLEAN_MIN_TEMP 170 \
        NOZZLE_CLEAN_START_POINT "{ {  10, 10, 3 }, {  10, 10, 3 } }" \
        NOZZLE_CLEAN_END_POINT "{ {  10, 20, 3 }, {  10, 20, 3 } }"
opt_enable REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER ADAPTIVE_FAN_SLOWING NO_FAN_SLOWING_IN_PID_TUNING \
           FILAMENT_WIDTH_SENSOR FILAMENT_LCD_DISPLAY PID_EXTRUSION_SCALING SOUND_MENU_ITEM \
           NOZZLE_AS_PROBE AUTO_BED_LEVELING_BILINEAR PREHEAT_BEFORE_LEVELING G29_RETRY_AND_RECOVER Z_MIN_PROBE_REPEATABILITY_TEST DEBUG_LEVELING_FEATURE \
           BABYSTEPPING BABYSTEP_XY BABYSTEP_ZPROBE_OFFSET BABYSTEP_ZPROBE_GFX_OVERLAY \
           PRINTCOUNTER NOZZLE_PARK_FEATURE NOZZLE_CLEAN_FEATURE SLOW_PWM_HEATERS PIDTEMPBED EEPROM_SETTINGS INCH_MODE_SUPPORT TEMPERATURE_UNITS_SUPPORT \
           Z_SAFE_HOMING ADVANCED_PAUSE_FEATURE PARK_HEAD_ON_PAUSE \
           HOST_KEEPALIVE_FEATURE HOST_ACTION_COMMANDS HOST_PROMPT_SUPPORT \
           LCD_INFO_MENU ARC_SUPPORT BEZIER_CURVE_SUPPORT EXTENDED_CAPABILITIES_REPORT AUTO_REPORT_TEMPERATURES \
           SDSUPPORT SDCARD_SORT_ALPHA AUTO_REPORT_SD_STATUS EMERGENCY_PARSER SOFT_RESET_ON_KILL SOFT_RESET_VIA_SERIAL
exec_test $1 $2 "Re-ARM with NOZZLE_AS_PROBE and many features." "$3"

# clean up
restore_configs
