#!/usr/bin/env bash
#
# Build tests for AVR ATmega2560
#

# exit on first failure
set -e

#
# Build with the default configurations
#
#restore_configs
#exec_test $1 $2 "Default Configuration" "$3"

#
# Test a probeless build of AUTO_BED_LEVELING_UBL, with lots of extruders
#
use_example_configs AnimationExample
opt_set MOTHERBOARD BOARD_AZTEEG_X3_PRO LCD_LANGUAGE fr SAVED_POSITIONS 4 \
        EXTRUDERS 5 TEMP_SENSOR_1 1 TEMP_SENSOR_2 5 TEMP_SENSOR_3 20 TEMP_SENSOR_4 1000 TEMP_SENSOR_BED 1
opt_enable AUTO_BED_LEVELING_UBL RESTORE_LEVELING_AFTER_G28 DEBUG_LEVELING_FEATURE G26_MESH_VALIDATION ENABLE_LEVELING_FADE_HEIGHT SKEW_CORRECTION \
           REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER LIGHTWEIGHT_UI STATUS_MESSAGE_SCROLLING SHOW_CUSTOM_BOOTSCREEN BOOT_MARLIN_LOGO_SMALL \
           SDSUPPORT SDCARD_SORT_ALPHA USB_FLASH_DRIVE_SUPPORT AUTO_REPORT_SD_STATUS SCROLL_LONG_FILENAMES MEDIA_MENU_AT_TOP \
           EEPROM_SETTINGS EEPROM_CHITCHAT GCODE_MACROS CUSTOM_MENU_MAIN FREEZE_FEATURE CANCEL_OBJECTS SOUND_MENU_ITEM \
           MULTI_NOZZLE_DUPLICATION CLASSIC_JERK LIN_ADVANCE EXTRA_LIN_ADVANCE_K QUICK_HOME \
           LCD_SET_PROGRESS_MANUALLY PRINT_PROGRESS_SHOW_DECIMALS SHOW_REMAINING_TIME \
           BABYSTEPPING BABYSTEP_XY NANODLP_Z_SYNC I2C_POSITION_ENCODERS M114_DETAIL
exec_test $1 $2 "Azteeg X3 Pro | EXTRUDERS 5 | RRDFGSC | UBL | LIN_ADVANCE ..." "$3"

#
# Add a Sled Z Probe, use UBL Cartesian moves, use Japanese language
#
use_example_configs AnimationExample
opt_set MOTHERBOARD BOARD_AZTEEG_X3_PRO LCD_LANGUAGE jp_kana \
        EXTRUDERS 5 TEMP_SENSOR_1 1 TEMP_SENSOR_2 5 TEMP_SENSOR_3 20 TEMP_SENSOR_4 1000 TEMP_SENSOR_BED 1
opt_enable REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER LIGHTWEIGHT_UI SHOW_CUSTOM_BOOTSCREEN BOOT_MARLIN_LOGO_SMALL \
           LCD_SET_PROGRESS_MANUALLY PRINT_PROGRESS_SHOW_DECIMALS SHOW_REMAINING_TIME STATUS_MESSAGE_SCROLLING SCROLL_LONG_FILENAMES \
           SDSUPPORT SDCARD_SORT_ALPHA NO_SD_AUTOSTART USB_FLASH_DRIVE_SUPPORT CANCEL_OBJECTS \
           Z_PROBE_SLED AUTO_BED_LEVELING_UBL UBL_HILBERT_CURVE RESTORE_LEVELING_AFTER_G28 DEBUG_LEVELING_FEATURE G26_MESH_VALIDATION ENABLE_LEVELING_FADE_HEIGHT \
           EEPROM_SETTINGS EEPROM_CHITCHAT GCODE_MACROS CUSTOM_MENU_MAIN \
           MULTI_NOZZLE_DUPLICATION CLASSIC_JERK LIN_ADVANCE QUICK_HOME \
           NANODLP_Z_SYNC I2C_POSITION_ENCODERS M114_DETAIL \
           SKEW_CORRECTION SKEW_CORRECTION_FOR_Z SKEW_CORRECTION_GCODE \
           BABYSTEPPING BABYSTEP_XY BABYSTEP_ZPROBE_OFFSET DOUBLECLICK_FOR_Z_BABYSTEPPING BABYSTEP_HOTEND_Z_OFFSET BABYSTEP_DISPLAY_TOTAL
opt_disable SEGMENT_LEVELED_MOVES
exec_test $1 $2 "Azteeg X3 Pro | EXTRUDERS 5 | RRDFGSC | UBL | LIN_ADVANCE | Sled Probe | Skew | JP-Kana | Babystep offsets ..." "$3"


#
# 5 runout sensors with distinct states
#
restore_configs
opt_set MOTHERBOARD BOARD_AZTEEG_X3_PRO NUM_SERVOS 1 \
        EXTRUDERS 5 TEMP_SENSOR_1 1 TEMP_SENSOR_2 1 TEMP_SENSOR_3 1 TEMP_SENSOR_4 1 \
        NUM_RUNOUT_SENSORS 5 FIL_RUNOUT2_PIN 44 FIL_RUNOUT3_PIN 45 FIL_RUNOUT4_PIN 46 FIL_RUNOUT5_PIN 47 \
        FIL_RUNOUT3_STATE HIGH
opt_enable VIKI2 BOOT_MARLIN_LOGO_ANIMATED SDSUPPORT AUTO_REPORT_SD_STATUS \
           Z_PROBE_SERVO_NR Z_SERVO_ANGLES DEACTIVATE_SERVOS_AFTER_MOVE AUTO_BED_LEVELING_3POINT DEBUG_LEVELING_FEATURE \
           EEPROM_SETTINGS EEPROM_CHITCHAT M114_DETAIL AUTO_REPORT_POSITION \
           NO_VOLUMETRICS EXTENDED_CAPABILITIES_REPORT AUTO_REPORT_TEMPERATURES AUTOTEMP G38_PROBE_TARGET JOYSTICK \
           DIRECT_STEPPING DETECT_BROKEN_ENDSTOP \
           FILAMENT_RUNOUT_SENSOR NOZZLE_PARK_FEATURE ADVANCED_PAUSE_FEATURE Z_SAFE_HOMING FIL_RUNOUT3_PULLUP
exec_test $1 $2 "Multiple runout sensors (x5) | Distinct runout states" "$3"


#
# Mixing Extruder with 5 steppers, Greek
#
restore_configs
opt_set MOTHERBOARD BOARD_AZTEEG_X3_PRO MIXING_STEPPERS 5 LCD_LANGUAGE ru \
        NUM_RUNOUT_SENSORS E_STEPPERS REDUNDANT_PART_COOLING_FAN 1 \
        FIL_RUNOUT2_PIN 16 FIL_RUNOUT3_PIN 17 FIL_RUNOUT4_PIN 4 FIL_RUNOUT5_PIN 5
opt_enable MIXING_EXTRUDER GRADIENT_MIX GRADIENT_VTOOL CR10_STOCKDISPLAY \
           USE_CONTROLLER_FAN CONTROLLER_FAN_EDITABLE CONTROLLER_FAN_IGNORE_Z \
           FILAMENT_RUNOUT_SENSOR ADVANCED_PAUSE_FEATURE NOZZLE_PARK_FEATURE
exec_test $1 $2 "Azteeg X3 | Mixing Extruder (x5) | Gradient Mix | Greek" "$3"

#
# Test SPEAKER with BOARD_BQ_ZUM_MEGA_3D and BQ_LCD_SMART_CONTROLLER
#
#restore_configs
#opt_set MOTHERBOARD BOARD_BQ_ZUM_MEGA_3D \
#        LCD_FEEDBACK_FREQUENCY_DURATION_MS 10 LCD_FEEDBACK_FREQUENCY_HZ 100
#opt_enable BQ_LCD_SMART_CONTROLLER SPEAKER

#
# Enable COREXY
#
#restore_configs
#opt_enable COREXY
#exec_test $1 $2 "Stuff" "$3"

######## Other Standard LCD/Panels ##############
#
# ULTRA_LCD
#
#restore_configs
#opt_enable ULTRA_LCD
#exec_test $1 $2 "Stuff" "$3"
#
# DOGLCD
#
#restore_configs
#opt_enable DOGLCD
#exec_test $1 $2 "Stuff" "$3"
#
# MAKRPANEL
# Needs to use Melzi and Sanguino hardware
#
#restore_configs
#opt_enable MAKRPANEL
#exec_test $1 $2 "Stuff" "$3"
#
# REPRAP_DISCOUNT_SMART_CONTROLLER, SDSUPPORT, BABYSTEPPING, RIGIDBOARD_V2, and DAC_MOTOR_CURRENT_DEFAULT
#
#restore_configs
#opt_set MOTHERBOARD BOARD_RIGIDBOARD_V2
#opt_enable REPRAP_DISCOUNT_SMART_CONTROLLER SDSUPPORT BABYSTEPPING DAC_MOTOR_CURRENT_DEFAULT
#exec_test $1 $2 "Stuff" "$3"
# #
# G3D_PANEL with SDCARD_SORT_ALPHA and STATUS_MESSAGE_SCROLLING
#
#restore_configs
#opt_enable G3D_PANEL SDSUPPORT SDCARD_SORT_ALPHA STATUS_MESSAGE_SCROLLING SCROLL_LONG_FILENAMES
#opt_set SDSORT_GCODE true SDSORT_USES_RAM true SDSORT_USES_STACK true SDSORT_CACHE_NAMES true
#exec_test $1 $2 "Stuff" "$3"
#
# REPRAPWORLD_KEYPAD
#
# Cant find configuration details to get it to compile
#restore_configs
#opt_enable ULTRA_LCD REPRAPWORLD_KEYPAD REPRAPWORLD_KEYPAD_MOVE_STEP
#exec_test $1 $2 "Stuff" "$3"
#
# RA_CONTROL_PANEL
#
#restore_configs
#opt_enable RA_CONTROL_PANEL PINS_DEBUGGING
#exec_test $1 $2 "Stuff" "$3"

######## I2C LCD/PANELS ##############
#
# !!!ATTENTION!!!
# Most I2C configurations are failing at the moment because they require
# a different Liquid Crystal library "LiquidTWI2".
#
# LCD_SAINSMART_I2C_1602
#
#restore_configs
#opt_enable LCD_SAINSMART_I2C_1602
#exec_test $1 $2 "Stuff" "$3"
#
# LCD_I2C_PANELOLU2
#
#restore_configs
#opt_enable LCD_I2C_PANELOLU2
#exec_test $1 $2 "Stuff" "$3"
#
# LCD_I2C_VIKI
#
#restore_configs
#opt_enable LCD_I2C_VIKI
#exec_test $1 $2 "Stuff" "$3"
#
# LCM1602
#
#restore_configs
#opt_enable LCM1602
#exec_test $1 $2 "Stuff" "$3"

#
# Test Laser features with 12864 LCD
#
restore_configs
opt_set MOTHERBOARD BOARD_RAMPS_14_EFB EXTRUDERS 0 LCD_LANGUAGE en TEMP_SENSOR_COOLER 1 TEMP_SENSOR_1 0 SERIAL_PORT_2 2 \
        DEFAULT_AXIS_STEPS_PER_UNIT '{ 80, 80, 400 }' \
        DEFAULT_MAX_FEEDRATE '{ 300, 300, 5 }' \
        DEFAULT_MAX_ACCELERATION '{ 3000, 3000, 100 }' \
        MANUAL_FEEDRATE '{ 50*60, 50*60, 4*60 }' \
        AXIS_RELATIVE_MODES '{ false, false, false }'
opt_enable REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER SDSUPPORT EEPROM_SETTINGS EEPROM_BOOT_SILENT EEPROM_AUTO_INIT \
           LASER_FEATURE AIR_EVACUATION AIR_EVACUATION_PIN AIR_ASSIST AIR_ASSIST_PIN LASER_COOLANT_FLOW_METER MEATPACK_ON_SERIAL_PORT_1

exec_test $1 $2 "REPRAP MEGA2560 RAMPS | Laser Feature | Air Evacuation | Air Assist | Cooler | Flowmeter | 12864 LCD | meatpack | SERIAL_PORT_2 " "$3"

#
# Test Laser features with 44780 LCD
#
restore_configs
opt_set MOTHERBOARD BOARD_RAMPS_14_EFB EXTRUDERS 0 LCD_LANGUAGE en TEMP_SENSOR_COOLER 1 TEMP_SENSOR_1 0 \
        DEFAULT_AXIS_STEPS_PER_UNIT '{ 80, 80, 400 }' \
        DEFAULT_MAX_FEEDRATE '{ 300, 300, 5 }' \
        DEFAULT_MAX_ACCELERATION '{ 3000, 3000, 100 }' \
        MANUAL_FEEDRATE '{ 50*60, 50*60, 4*60 }' \
        AXIS_RELATIVE_MODES '{ false, false, false }'
opt_enable REPRAP_DISCOUNT_SMART_CONTROLLER SDSUPPORT EEPROM_SETTINGS EEPROM_BOOT_SILENT EEPROM_AUTO_INIT \
           LASER_FEATURE AIR_EVACUATION AIR_EVACUATION_PIN AIR_ASSIST AIR_ASSIST_PIN LASER_COOLANT_FLOW_METER I2C_AMMETER

exec_test $1 $2 "REPRAP MEGA2560 RAMPS | Laser Feature | Air Evacuation | Air Assist | Cooler | Flowmeter | 44780 LCD " "$3"

#
# Language files test with REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER
#
#restore_configs
#opt_enable REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER SDSUPPORT
#for lang in an bg ca cz da de el el_gr en es eu fi fr gl hr hu it jp_kana nl pl pt pt_br ro ru sk sv tr uk vi zh_CN zh_TW test; do opt_set LCD_LANGUAGE $lang; echo "compile with language $lang ..."; exec_test $1 $2 "Stuff" "$3"; done
#
#restore_configs
#opt_enable REPRAP_DISCOUNT_SMART_CONTROLLER SDSUPPORT
#for lang in an bg ca cz da de el el_gr en es eu fi fr gl hr hu it jp_kana nl pl pt pt_br ro ru sk sv tr uk vi zh_CN zh_TW test; do opt_set LCD_LANGUAGE $lang; echo "compile with language $lang ..."; exec_test $1 $2 "Stuff" "$3"; done

######## Example Configurations ##############
#
# Test a basic DUAL_X_CARRIAGE configuration
#
use_example_configs Formbot/T_Rex_3
exec_test $1 $2 "Formbot/T_Rex_3 example configuration." "$3"

#
# BQ Hephestos 2
#restore_configs
#use_example_configs BQ/Hephestos_2
#exec_test $1 $2 "Stuff" "$3"

#
# Makibox Config  need to check board type for Teensy++ 2.0
#
#use_example_configs makibox
#exec_test $1 $2 "Stuff" "$3"

#
# tvrrug Config need to check board type for sanguino atmega644p
#
#use_example_configs tvrrug/Round2
#exec_test $1 $2 "Stuff" "$3"

# clean up
restore_configs
