#!/usr/bin/env bash
#
# Build tests for MKS Robin nano
# (STM32F1 genericSTM32F103VE)
#

# exit on first failure
set -e

#
# MKS Robin nano v1.2 Emulated DOGM FSMC
#
use_example_configs Mks/Robin
opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO
exec_test $1 $2 "MKS Robin nano v1.2 Emulated DOGM FSMC" "$3"

#
# MKS Robin v2 nano Emulated DOGM SPI
# (Robin v2 nano has no FSMC interface)
#
use_example_configs Mks/Robin
opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO_V2
opt_disable TFT_INTERFACE_FSMC
opt_enable TFT_INTERFACE_SPI
exec_test $1 $2 "MKS Robin v2 nano Emulated DOGM SPI" "$3"

#
# MKS Robin nano v1.2 LVGL FSMC
#
# use_example_configs Mks/Robin
# opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO
# opt_disable TFT_CLASSIC_UI TFT_COLOR_UI TOUCH_SCREEN TFT_RES_320x240
# opt_enable TFT_LVGL_UI TFT_RES_480x320
# exec_test $1 $2 "MKS Robin nano v1.2 LVGL FSMC" "$3"

#
# MKS Robin v2 nano LVGL SPI
# (Robin v2 nano has no FSMC interface)
#
# use_example_configs Mks/Robin
# opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO_V2
# opt_disable TFT_INTERFACE_FSMC TFT_COLOR_UI TOUCH_SCREEN TFT_RES_320x240
# opt_enable TFT_INTERFACE_SPI TFT_LVGL_UI TFT_RES_480x320
# exec_test $1 $2 "MKS Robin v2 nano LVGL SPI" "$3"

#
# MKS Robin v2 nano New Color UI 480x320 SPI
# (Robin v2 nano has no FSMC interface)
#
use_example_configs Mks/Robin
opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO_V2
opt_disable TFT_INTERFACE_FSMC TFT_RES_320x240
opt_enable TFT_INTERFACE_SPI TFT_RES_480x320
exec_test $1 $2 "MKS Robin v2 nano New Color UI 480x320 SPI" "$3"

#
# MKS Robin v2 nano LVGL SPI + TMC
# (Robin v2 nano has no FSMC interface)
#
# use_example_configs Mks/Robin
# opt_set MOTHERBOARD BOARD_MKS_ROBIN_NANO_V2 X_DRIVER_TYPE TMC2209 Y_DRIVER_TYPE TMC2209
# opt_disable TFT_INTERFACE_FSMC TFT_COLOR_UI TOUCH_SCREEN TFT_RES_320x240
# opt_enable TFT_INTERFACE_SPI TFT_LVGL_UI TFT_RES_480x320
# exec_test $1 $2 "MKS Robin v2 nano LVGL SPI + TMC" "$3"

# cleanup
restore_configs
