#!/usr/bin/env bash
#
# Build tests for STM32F407VGT6 BigTreeTech BTT002 V1.0
#

# exit on first failure
set -e

#
# Build with the default configurations
#
restore_configs
opt_set MOTHERBOARD BOARD_BTT_BTT002_V1_0 \
        SERIAL_PORT 1 \
        X_DRIVER_TYPE TMC2209 \
        Y_DRIVER_TYPE TMC2130
exec_test $1 $2 "BigTreeTech BTT002 Default Configuration plus TMC steppers" "$3"

#
# A test with Probe Temperature Compensation enabled
#
use_example_configs Prusa/MK3S-BigTreeTech-BTT002
exec_test $1 $2 "BigTreeTech BTT002 with Prusa MK3S and related options" "$3"

# clean up
restore_configs
