#!/usr/bin/env bash
#
# Build tests for STM32F103RET6_creality
#

# exit on first failure
set -e

#
# Build with configs included in the PR
#
use_example_configs "Creality/Ender-3 V2"
opt_enable MARLIN_DEV_MODE
exec_test $1 $2 "Ender 3 v2" "$3"

use_example_configs "Creality/Ender-3 V2"
opt_disable CLASSIC_JERK
opt_add SDCARD_EEPROM_EMULATION
opt_set TEMP_SENSOR_BED 0
exec_test $1 $2 "Ender 3 v2, SD EEPROM, no CLASSIC_JERK, no Bed" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_CREALITY_V452 SERIAL_PORT 1
opt_disable NOZZLE_TO_PROBE_OFFSET
opt_enable NOZZLE_AS_PROBE Z_SAFE_HOMING Z_MIN_PROBE_USES_Z_MIN_ENDSTOP_PIN \
           PROBE_ACTIVATION_SWITCH PROBE_TARE PROBE_TARE_ONLY_WHILE_INACTIVE
exec_test $1 $2 "Creality V4.5.2 PROBE_ACTIVATION_SWITCH, Probe Tare" "$3"

# clean up
restore_configs
