# Adafruit SCD30 [![Build Status](https://github.com/adafruit/Adafruit_SCD30/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_SCD30/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_SCD30/html/index.html)


This is the Adafruit SCD30 CO2, Temperature, and Humidity Sensor Library for Arduino

Tested and works great with the [Adafruit SCD30 Breakout Board](https://www.adafruit.com/products/4867):

[<img src="assets/board.png?raw=true" width="500px">](https://www.adafruit.com/products/4867)

Adafruit invests time and resources providing this open source code, please support Adafruit and open-source hardware by purchasing products from Adafruit!

# Installation
To install, use the Arduino Library Manager and search for "Adafruit SCD30" and install the library.

## Dependencies
 * [Adafruit BusIO](https://github.com/adafruit/Adafruit_BusIO)
 * [Adafruit Unified Sensor Driver](https://github.com/adafruit/Adafruit_Sensor)
 * [Adafruit SSD1306](https://github.com/adafruit/Adafruit_SSD1306)
p
# Contributing

Contributions are welcome! Please read our [Code of Conduct](https://github.com/adafruit/Adafruit_SCD30/blob/master/code-of-conduct.md)
before contributing to help this project stay welcoming.

## Documentation and doxygen
Documentation is produced by doxygen. Contributions should include documentation for any new code added.

Some examples of how to use doxygen can be found in these guide pages:

https://learn.adafruit.com/the-well-automated-arduino-library/doxygen

https://learn.adafruit.com/the-well-automated-arduino-library/doxygen-tips

## Formatting and clang-format
This library uses [`clang-format`](https://releases.llvm.org/download.html) to standardize the formatting of `.cpp` and `.h` files. 
Contributions should be formatted using `clang-format`:

The `-i` flag will make the changes to the file.
```bash
clang-format -i *.cpp *.h
```
If you prefer to make the changes yourself, running `clang-format` without the `-i` flag will print out a formatted version of the file. You can save this to a file and diff it against the original to see the changes.

Note that the formatting output by `clang-format` is what the automated formatting checker will expect. Any diffs from this formatting will result in a failed build until they are addressed. Using the `-i` flag is highly recommended.

### clang-format resources
  * [Binary builds and source available on the LLVM downloads page](https://releases.llvm.org/download.html)
  * [Documentation and IDE integration](https://clang.llvm.org/docs/ClangFormat.html)

## About this Driver
Written by Bryan Siepert for Adafruit Industries.
BSD license, check license.txt for more information
All text above must be included in any redistribution
